**REQUEST FOR QUOTATION  
SPECIFICATION OF STANDARD GOODS**

**Procurement No:** **15-G003-21**

## Specification

### Background

The Ministry of Internal Affairs (MIA) is working with the Ministry of Environment, Lands and Agricultural Development (MELAD) to focus on strengthening waste collections and management systems in South Tarawa. A key part of Urban Services is the provision of litter bins in public spaces. MIA is pleased to lead the procurement of public litter bins, in partnership with MELAD and the two urban councils on South Tarawa.

This project was part of NZMFAT program on Urban Development (UDP) that focus on Solid Waste Management Project (SWaMP). This is Phase 2 of the UDP SWaMP program which merely builds on the previous phase with an objective - ‘Effective and Sustainable SWM supporting the well-being of communities. Expected outcomes includes but not limited to;

1. I-Kiribati have greater awareness of the importance of Solid Waste Management and the connection to personal and environmental health
2. I-Kiribati have access to reliable solid waste management services
3. Kiribati has the necessary solid waste management governance, regulatory and operational capacities in-place
4. Improved management of solid waste materials entering Kiribati
5. I-Kiribati participate in solid waste management
6. Kiribati maintain its solid waste management services in a sustainable manner
7. Reduced amount of solid waste being improperly disposed of in Kiribati
8. Improved health of communities and reduced detriment to environment through effective SWM

In supporting the above deliverable outputs, the Ministry of Internal Affairs is proposing to procure and installing of public 220 litter bins. However the number of bins to be procured will be determined in the Contract of Agreement with the supplier and may change subject to unit prize provided (depending on the quotation/prize of material required).

### Requirements

All supporting documentation must be in English. The costing must complete and inclusive of freight cost, installation cost, relevant taxes, and other relevant costs.

### Installation services

Supplier should provide details of installation that inclusive of design, materials to be used, costings, timeframes and other relevant installation details

**120L Wheelie Bin Lock Stand Installation**



1. **Material Description**

* 35 x 35 x 3mm SHS post
* 200 x 200 x 5mm base plate
* Hot dipped galvanized steel fitted with deadbolt locks
* Bolt-down stand height 890mm
* With a universal keyed lock

1. **Installation**

* Install a 700 x 600 x 100 mm concrete pad for unpaved areas
* Install wheelie bin lock stand on concrete pad and existing pavement with 4No. M10 galvanized chemset anchors to fit predrilled holes in base plate
* Refer to installation details for more information

1. Concrete quantity

* For a 20Mpa concrete strength with a 1concrete;2sand;3aggregate mix ratio requires;
* 55.44bags of 40kg cement;
* 3.54 cubic meters of sand, and
* 4.16 cubic meters of aggregate

****

### Delivery Time

Suppliers should have filled in their delivery time and specified whether there are materials available on hand or need purchasing from overseas.

## Description of the Goods

Litter bins shall be procured and installed. Suppliers shall list all the items and materials required for the tender with the quotes. Note that your quotation must be VAT inclusive for VAT registered companies

|  |  |  |  |
| --- | --- | --- | --- |
| **Description** | **SIZE** | **SAMPLE TYPES** | **Quantity** |
| - Fitted with deadbolt locks keyed alike  - 35x35x3 SHS post  - 200 x 200 x 5mm base  - Hot dip galvanized | **120L Wheelie Bin Lock Stand** |  | **120** |
| Dark/light green with lid  120HDPE  Manufactured to AS4123  Full white embossed design on front of bin (attached)  All bins to have wheels | **120L Wheelie Bins** |  | **120** |
| Dark/light green with lid & stand/bolted holes of 50L HDPE manufactured to AS4123 Full white embossed design on front of bin  All bins without wheels | **50L Wheelie Bins** |  | **50** |
| Galvanized/stainless outdoor trash bin of 50L with Full black embossed design on front of bin  All bins without wheels | **50L Stainless Bins** |  | **50** |

|  |  |  |
| --- | --- | --- |
| **Pricing Table (pls complete this table)** | | |
| **1.       Bin Pricing** | **Cost per Unit** | **Cost over 100 Units** |
| **120L Wheelie Bin**  -          Dark green with lid  -          HDPE  -          Manufactured to AS4123  -          With wheels  -          Hot stamp |  |  |
| **120L Wheelie Bin Lock Stand**  -          Hot dip galvanised stand  -          35x35x35 SHS post  -          200x200x5mm plate base  -          Universal keyed padlock 50mm brass |  |  |
| *other bins including stainless steel or other designs* |  |  |
| 2.       Freight Costs |  |  |
| ***Shipping to Port Betio, Tarawa*** |  |  |
| 3.       Installation on South Tarawa |  |  |
| ***Installation cost to manufacturers standard*** |  |  |
| **TOTAL** | **AUD** | **AUD** |